**Date Submitted: 11/11/2019**

**------------------------------------------------------------------------------------**

**Task 01:**

Youtube Link: N/A

**Modified Schematic (if applicable): N/A**

**Modified Code:**

//----------------------------------------

// BIOS header files

//----------------------------------------

**#include** <xdc/std.h> //mandatory - have to include first, for BIOS types

**#include** <ti/sysbios/BIOS.h> //mandatory - if you call APIs like BIOS\_start()

**#include** <xdc/runtime/Log.h> //needed for any Log\_info() call

**#include** <xdc/cfg/global.h> //header file for statically defined objects/handles

**#include** <xdc/runtime/Timestamp.h> // used for Timestamp() calls

//------------------------------------------

// TivaWare Header Files

//------------------------------------------

**#include** <stdint.h>

**#include** <stdbool.h>

**#include** "inc/hw\_types.h"

**#include** "inc/hw\_memmap.h"

**#include** "driverlib/sysctl.h"

**#include** "driverlib/gpio.h"

**#include** "inc/hw\_ints.h"

**#include** "driverlib/interrupt.h"

**#include** "driverlib/timer.h"

//----------------------------------------

// Prototypes

//----------------------------------------

**void** **hardware\_init**(**void**);

**void** **ledToggle**(**void**);

//---------------------------------------

// Globals

//---------------------------------------

**volatile** int16\_t i16ToggleCount = 0;

//---------------------------------------------------------------------------

// main()

//---------------------------------------------------------------------------

**void** **main**(**void**)

{

hardware\_init(); // init hardware via Xware

BIOS\_start();

}

//---------------------------------------------------------------------------

// hardware\_init()

//

// inits GPIO pins for toggling the LED

//---------------------------------------------------------------------------

**void** **hardware\_init**(**void**)

{

//Set CPU Clock to 40MHz. 400MHz PLL/2 = 200 DIV 5 = 40MHz

SysCtlClockSet(SYSCTL\_SYSDIV\_5|SYSCTL\_USE\_PLL|SYSCTL\_XTAL\_16MHZ|SYSCTL\_OSC\_MAIN);

// ADD Tiva-C GPIO setup - enables port, sets pins 1-3 (RGB) pins for output

SysCtlPeripheralEnable(SYSCTL\_PERIPH\_GPIOF);

GPIOPinTypeGPIOOutput(GPIO\_PORTF\_BASE, GPIO\_PIN\_1|GPIO\_PIN\_2|GPIO\_PIN\_3);

// Turn on the LED

GPIOPinWrite(GPIO\_PORTF\_BASE, GPIO\_PIN\_1|GPIO\_PIN\_2|GPIO\_PIN\_3, 4);

}

//---------------------------------------------------------------------------

// ledToggle()

//

// toggles LED on Tiva-C LaunchPad

//---------------------------------------------------------------------------

**void** **ledToggle**(**void**)

{

**static** uint32\_t ui32\_t0, ui32\_t1, ui32\_t2, ui32start, ui32stop, ui32delta; // used for Timestamp calculations

ui32\_t0 = Timestamp\_get32(); // calculate Timestamp() overhead (ui32\_t2)

ui32\_t1 = Timestamp\_get32();

ui32\_t2 = ui32\_t1 - ui32\_t0;

// LED values - 2=RED, 4=BLUE, 8=GREEN

**if**(GPIOPinRead(GPIO\_PORTF\_BASE, GPIO\_PIN\_2))

{

ui32start = Timestamp\_get32(); // get starting Timer snapshot for LED benchmark

GPIOPinWrite(GPIO\_PORTF\_BASE, GPIO\_PIN\_1|GPIO\_PIN\_2|GPIO\_PIN\_3, 0); // toggle GPIO/LED

ui32stop = Timestamp\_get32(); // get ending Timer snapshot for LED benchmark

ui32delta = ui32stop - ui32start - ui32\_t2; // calculate LED toggle benchmark

Log\_info1("LED BENCHMARK = [%u] TM4C CYCLES", ui32delta); // send LED benchmark to Log display

}

**else**

{

GPIOPinWrite(GPIO\_PORTF\_BASE, GPIO\_PIN\_2, 4);

}

i16ToggleCount += 1; // keep track of #toggles

Log\_info1("LED TOGGLED [%u] TIMES",i16ToggleCount); // send toggle count to UIA

}

**------------------------------------------------------------------------------------**